# GracoPd2kInt API

## Add-On Instructions (AOIs)

### PumpCtrl

Provides several inputs for controlling the PD2K proportioner (e.g. system mode, setpoints).

The enable input must be on for any other inputs to take effect. The boolean command inputs each function like execute inputs, meaning the command will automatically reset these once set to true.

The current control mode setting (pressure or flow) determines which of the setpoint inputs are written to the PD2K system. This switches automatically when the control mode is changed.

clearAlarm (INPUT BOOL)

  Clear alarm

completeJob (INPUT BOOL)

  Complete job

ctrlMode (INPUT BOOL)

  Ctrl mode SP (0=flow, 1=pressure)

enable (INPUT BOOL)

  Enable command

mix (INPUT BOOL)

  Goto mix

mixFill (INPUT BOOL)

  Goto mix fill

powerOff (INPUT BOOL)

  Power off

powerOn (INPUT BOOL)

  Power on

quickStop (INPUT BOOL)

  Goto quick stop

recipePurge (INPUT BOOL)

  Goto recipe purge

standby (INPUT BOOL)

  Goto standby

flowCtrlSP (INPUT DINT)

  Flow control setpoint (cc/min)

presCtrlSP (INPUT DINT)

  Pressure control setpoint (psi)

busy (OUTPUT BOOL)

  Command busy flag

valid (OUTPUT BOOL)

  Command valid flag

aborted (OUTPUT BOOL)

  Command aborted flag

error (OUTPUT BOOL)

  Command error flag

state (OUTPUT DINT)

  State code

moduleStatus (INOUT DINT[46])

  Data from module to PLC

moduleCmds (INOUT DINT[18])

  Data from PLC to module

#### State Codes

- 16#0000 - Idle

- 16#3XXX - Valid

- 16#9000 - Error, control mode could not be updated

### ReadAlarmInfo

Reads data from an alarm record.

indexNum (INPUT DINT)

  the chronological alarm index number to look up, where 0 is the most recent, and 199 is the 200th most recent.

execute (INPUT BOOL)

  executes the command.

code (INOUT STRING4)

  the code for the alarm.

dateTime (INOUT TypeDateTime)

  The date and time the alarm occurred.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadEventInfo

Reads data from an event record.

indexNum (INPUT DINT)

  the chronological event index number to look up, where 0 is the most recent, and 199 is the 200th most recent.

execute (INPUT BOOL)

  executes the command.

code (INOUT STRING4)

  the code for the event.

dateTime (INOUT TypeDateTime)

  The date and time the event occurred.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadFluidControlMode

Returns the current fluid control mode for the system.

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

mode (OUTPUT BOOL)

  The current fluid control mode value (false=flow control, true=pressure control).

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadGrandTotals

Returns the material grand total volume data.

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

materialA (OUTPUT DINT)

  the grand total volume of material A used, in gallons.

materialB (OUTPUT DINT)

  the grand total volume of material B used, in gallons.

materialC (OUTPUT DINT)

  the grand total volume of material C used, in gallons.

materialD (OUTPUT DINT)

  the grand total volume of material D used, in gallons.

materialABCD (OUTPUT DINT)

  the summed grand total of materials A, B, C, and D, in gallons.

solvent (OUTPUT DINT)

  the grand total volume of solvent used, in gallons.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadGunContents

Returns the recipe number of mixed material that is currently loaded in the specified gun number.

gunNum (INPUT DINT)

  The gun number to look up. The acceptable range is 1-3. If not in range, an error will be raised.

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[41])

  The module input data.

moduleCmds (INOUT DINT[22])

  The module output data.

recipeNum (OUTPUT DINT)

  The current recipe number. If the recipe is unknown (e.g. on startup), a value of 61 will be returned.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadGunPotLifeTime

Returns the remaining pot life time for a selected gun number if it is currently loaded and mixed.

This command is particularly useful if multiple guns are enabled.

gunNum (INPUT DINT)

  The gun number to look up. The acceptable range is 1-3.

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

remTimeStage1 (OUTPUT DINT)

  The remaining pot life time for stage 1 in seconds.

remTimeStage2 (OUTPUT DINT)

  The remaining pot life time for stage 2 in seconds.

remTimeStage3 (OUTPUT DINT)

  The remaining pot life time for stage 3 in seconds.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadJobInfo

Reads data from a job record.

indexNum (INPUT DINT)

  the chronological job index number to look up, where 0 is the most recent, and 199 is the 200th most recent.

execute (INPUT BOOL)

  executes the command.

userID (INOUT STRING9)

  the user ID used for the job.

dateTime (INOUT TypeDateTime)

  the completion date and time of the job record.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

jobNum (OUTPUT DINT)

  The actual job number of the record.

recipeNum (OUTPUT DINT)

  The recipe number used for the job.

sprayedVol (OUTPUT DINT)

  The sum of materials (A+B+C+D) used for the job in cc.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadPumpMaterial

Returns the material number currently loaded in the specified pump number.

pumpNum (INPUT DINT)

  The pump number to look up. The acceptable range is 1-4. If not in range, an error will be raised.

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

materialNum (OUTPUT DINT)

  The current material number. If the material is unknown (e.g. on startup), a value of 61 will be returned.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadRecipe

Returns the current configuration values for a recipe number.

recipeNum (INPUT DINT)

  the recipe number to read. The acceptable range is 0-60.

execute (INPUT BOOL)

  Executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

materialA (OUTPUT DINT)

  the current value for the first material number.

materialB (OUTPUT DINT)

  the current value for the second material number.

materialC (OUTPUT DINT)

  the current value for the third material number.

materialD (OUTPUT DINT)

  the current value for the fourth material number.

gunNum (OUTPUT DINT)

  the current value for the assigned gun number.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### ReadUserID

Returns the current user ID for the system.

The returned value is a string of up to 9 characters, not including a null terminator.

execute (INPUT BOOL)

  Executes the command

mixUnitNum (INPUT DINT)

  mix unit number (1-2)

userID (INOUT STRING9)

  The returned user ID

moduleStatus (INOUT DINT[46])

  The module input data

moduleCmds (INOUT DINT[18])

  The module output data

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### RecipeChange

Performs a recipe change operation.

execute (INPUT BOOL)

  executes the command.

recipeNum (INPUT DINT)

  The next recipe number to use.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, system must be powered on

- 16#8001 - Error, another recipe change is already in progress

- 16#8002 - Error, system alarm is active

- 16#8003 - Error, another operation is active

- 16#8004 - Error, alarm occurred

- 16#8005 - Error, unexpected system mode

- 16#8006 - Error, recipe change did not finish

- 16#8007 - Error, timeout waiting for system registers to become available

### SendDCS

Sends a dynamic command structure (DCS) message to the PD2K system.

For more information about DCS commands, see the system operation manual.

execute (INPUT BOOL)

  executes the command.

cmdID (INPUT DINT)

  the command number to send.

arg0 (INPUT DINT)

  argument 0.

arg1 (INPUT DINT)

  argument 1.

arg2 (INPUT DINT)

  argument 2.

arg3 (INPUT DINT)

  argument 3.

arg4 (INPUT DINT)

  argument 4.

arg5 (INPUT DINT)

  argument 5.

arg6 (INPUT DINT)

  argument 6.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

return0 (OUTPUT DINT)

  Return value 0 from the PD2K.

return1 (OUTPUT DINT)

  Return value 1 from the PD2K.

return2 (OUTPUT DINT)

  Return value 2 from the PD2K.

return3 (OUTPUT DINT)

  Return value 3 from the PD2K.

return4 (OUTPUT DINT)

  Return value 4 from the PD2K.

return5 (OUTPUT DINT)

  Return value 5 from the PD2K.

return6 (OUTPUT DINT)

  Return value 6 from the PD2K.

return7 (OUTPUT DINT)

  Return value 7 from the PD2K.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### StatusToUDT

Reads a PD2K module array into a structured UDT.

moduleStatus (INOUT DINT[46])

  The module input data.

statusUDT (INOUT TypePd3kStatus)

  The structured data from the device.

### WriteFluidControlMode

Sets the fluid control mode for the system.

mode (INPUT BOOL)

  the fluid control mode to set (false=flow control, true=pressure control).

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### WriteMaterialReadyFlag

Sets the flag used to signal that the upstream material management is loaded correctly prior to a recipe change.

This flag is only used when multiple materials for a pump are fed to the PD2K via a single valve at the inlet valve stack (i.e. a piggable system).

materialReadyFlag (INPUT BOOL)

  the new flag value (false=not ready, true=ready).

execute (INPUT BOOL)

  executes the command.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### WriteRecipe

Configures the values for a recipe number.

execute (INPUT BOOL)

  Executes the command.

recipeNum (INPUT DINT)

  the recipe number to configure. The acceptable range is 0-60.

materialA (INPUT DINT)

  the first material number to set.

materialB (INPUT DINT)

  the second material number to set.

materialC (INPUT DINT)

  the third material number to set.

materialD (INPUT DINT)

  the fourth material number to set.

moduleStatus (INOUT DINT[46])

  The module input data.

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

### WriteUserID

Sets the current user ID for the system.

The user ID can be up to 9 characters in length. The value sent to the PD2K will include a null terminator for a total of 10 characters. Only ASCII characters are supported.

execute (INPUT BOOL)

  Executes the command

userID (INOUT STRING9)

  The new user ID

moduleStatus (INOUT DINT[46])

  The module input data

moduleCmds (INOUT DINT[18])

  The module output data.

busy (OUTPUT BOOL)

  The busy command flag

done (OUTPUT BOOL)

  The done command flag

aborted (OUTPUT BOOL)

  The aborted command flag

error (OUTPUT BOOL)

  The error command flag

state (OUTPUT DINT)

  State data for the command

#### State Codes

- 16#1xxx - Busy

- 16#2000 - Done

- 16#4000 - Aborted, command overwritten by another process

- 16#8000 - Error, invalid command ID

- 16#8001 - Error, timeout waiting for DCS registers to become available

- 16#8002 - Error, command unsuccessful

- 16#8003 - Error, timeout waiting for acknowledge from PD2K

## User-Defined Types (UDTs)

### TypePd3kPumpStatusFlags

Status flags for a PD3K pump.

off (BOOL)

  pump is off.

standby (BOOL)

  pump is in standby.

busy (BOOL)

  pump is busy.

flushing (BOOL)

  pump is flushing.

priming (BOOL)

  pump is priming.

### TypePd3kStatus

Status data read from a PD3K system.

standby (BOOL)

  in standby

eventFlag (BOOL)

  event flag

gun1TriggerStatus (BOOL)

  gun 1 trigger status (1 = on)

gun2TriggerStatus (BOOL)

  gun 2 trigger status(1 = on)

gun3TriggerStatus (BOOL)

  gun 3 trigger status(1 = on)

safetyInterlockStatus (BOOL)

  safety interlock status

systemMode (DINT)

  system mode

systemModeFlags (TypePd3kSystemModeFlags)

  system mode flags

actualMixFlowPressure (DINT)

  actual mix flow/pressure (cc/min in flow mode, psi in pressure mode)

actualMixRatioA (DINT)

  actual mix ratio A

actualMixRatioB (DINT)

  actual mix ratio B

actualMixRatioC (DINT)

  actual mix ratio C

actualMixRatioD (DINT)

  actual mix ratio D

actualMixPotLifeRemStage1 (DINT)

  actual pot life remaining stage 1

actualMixPotLifeRemStage2 (DINT)

  actual pot life remaining stage 2

actualMixPotLifeRemStage3 (DINT)

  actual pot life remaining stage 3

activeGunNum (DINT)

  active gun number

jobNum (DINT)

  job number

jobTotalSprayedVol (DINT)

  job total sprayed volume (cc)

jobSolventVol (DINT)

  job solvent volume (cc)

activeRecipeNum (DINT)

  active recipe number

activeMaterialA (DINT)

  active material A

activeMaterialB (DINT)

  active material B

activeMaterialC (DINT)

  active material C

activeMaterialD (DINT)

  active material D

activeRecipeRatioA (DINT)

  active recipe ratio A

activeRecipeRatioB (DINT)

  active recipe ratio B

activeRecipeRatioC (DINT)

  active recipe ratio C

activeRecipeRatioD (DINT)

  active recipe ratio D

pump1Status (DINT)

  pump 1 status

pump1StatusFlags (TypePd3kPumpStatusFlags)

  pump 1 status flags

pump2Status (DINT)

  pump 2 status

pump2StatusFlags (TypePd3kPumpStatusFlags)

  pump 2 status flags

pump3Status (DINT)

  pump 3 status

pump3StatusFlags (TypePd3kPumpStatusFlags)

  pump 3 status flags

pump4Status (DINT)

  pump 4 status

pump4StatusFlags (TypePd3kPumpStatusFlags)

  pump 4 status flags

actualPump1Flow (DINT)

  actual pump 1 flow rate (cc/min)

actualPump2Flow (DINT)

  actual pump 2 flow rate (cc/min)

actualPump3Flow (DINT)

  actual pump 3 flow rate (cc/min)

actualPump4Flow (DINT)

  actual pump 4 flow rate (cc/min)

actualPump1Pressure (DINT)

  actual pump 1 pressure (psi)

actualPump2Pressure (DINT)

  actual pump 2 pressure (psi)

actualPump3Pressure (DINT)

  actual pump 3 pressure (psi)

actualPump4Pressure (DINT)

  actual pump 4 pressure (psi)

dcsReturn0 (DINT)

  DCS return 0

dcsReturn1 (DINT)

  DCS return 1

dcsReturn2 (DINT)

  DCS return 2

dcsReturn3 (DINT)

  DCS return 3

dcsReturn4 (DINT)

  DCS return 4

dcsReturn5 (DINT)

  DCS return 5

dcsReturn6 (DINT)

  DCS return 6

dcsReturn7 (DINT)

  DCS return 7

dcsAck (DINT)

  DCS acknowledge

### TypePd3kSystemModeFlags

Flags for the PD3K system mode.

pumpOff (BOOL)

  pump off

colorChange (BOOL)

  color change enabled

colorChangePurgeA (BOOL)

  color change purging component A

colorChangePurgeB (BOOL)

  color change purging component B

colorChangePurgeC (BOOL)

  color change purging component C

colorChangePurgeD (BOOL)

  color change purging component D

colorChangeFilling (BOOL)

  color change filling

mixFillStage1 (BOOL)

  mix fill stage 1

mixFillStage2 (BOOL)

  mix fill stage 2

mixFillStage3 (BOOL)

  mix fill stage 3

mix (BOOL)

  mixing

mixIdle (BOOL)

  mix idle

purgeA (BOOL)

  purging component A

purgeB (BOOL)

  purging component B

purgeC (BOOL)

  purging component C

purgeD (BOOL)

  purging component D

standbyMixReady (BOOL)

  standby mix ready

standbyFillReady (BOOL)

  standby fill ready

standbyMixNotReady (BOOL)

  standby mix not ready

standbyAlarm (BOOL)

  standby alarm

lineFillingFlushing (BOOL)

  line is filling or flushing

pumpPrimeFlush (BOOL)

  pump is priming or flushing

maintCalibration (BOOL)

  maintenance/calibration

mixSolventPush (BOOL)

  mix solvent push